**Water Supply Network Works**

1. All design of water supply network works shall be in accordance with the **Water Supply Code of Australia, South East Queensland Service Providers Edition Version 1.3 (August 2019), Part 1: Planning and Design** and **Part 3: Drawings**.
2. All construction of water supply network works shall be in accordance with the **Water Supply Code of Australia, South East Queensland Service Providers Edition Version 1.3 (August 2019), Part 2: Construction** and **Part 3: Drawings**.
3. All products and materials used in construction of water supply network works shall be in accordance with the **South East Queensland Code Accepted Civil Infrastructure Products and Material List**, and the most recent version of the List in effect at the date of the construction Pre-Start Meeting.
4. Construction works shall be supervised by an engineer who has RPEQ registration. Works not complying with this requirement will not be permitted to connect into Unitywater's water supply network.
5. All Live Works associated with the water supply network shall be carried out at the Developer's cost by quotation request to Unitywater Private Works only.
6. The Constructor shall verify the location and depth of existing services with relevant asset owners and authorities before commencing works.
7. Prior to commencement of any Variation Works, the Constructor must first obtain approval from the Registered Major Connections Certifier.

**Gravity Sewerage Network Works**

1. All design of gravity sewerage network works shall be in accordance with the **Gravity Sewerage Code of Australia, South East Queensland Service Providers Edition Version 2.0 (July 2019), Part 1: Planning and Design** and **Part 3: Drawings**.
2. All construction of gravity sewerage network works shall be in accordance with the **Gravity Sewerage Code of Australia, South East Queensland Service Providers Edition Version 2.0 (July 2019), Part 2: Construction** and **Part 3: Drawings**.
3. All products and materials used in construction of gravity sewerage network works shall be in accordance with the **South East Queensland Code Accepted Civil Infrastructure Products and Material List**, and the most recent version of the List in effect at the date of the construction Pre-Start Meeting.
4. Construction works shall be supervised by an engineer who has RPEQ registration. Works not complying with this requirement will not be permitted to connect into Unitywater's sewerage network.
5. All Live Works associated with the sewerage network shall be carried out at the Developer's cost, either:
   1. By the Constructor, for ‘minor’ sewerage connection works, defined in the A&C Manual under section Pre-Start Meeting, under the inspection of the Construction Certifier who shall follow the Planned Network Intervention process, or
   2. By quotation request to Unitywater Private Works, for sewerage connection works not meeting the criteria for classification as ‘minor’.
6. The Constructor shall verify the location and depth of existing services with relevant asset owners and authorities before commencing works.
7. Prior to commencement of any Variation Works, the Constructor must first obtain approval from the Registered Major Connections Certifier.